Example:
Version	SKRZ12030
Serial No. / Production-Nr.	11151810089
Type / Axletype	ID1-	ID1-SNK3020
Perm. Axle cap. / Achslast Stat.	kg	12000 kg
ID 3	ID3-	ID3-11379
Test Report / TDB-Nr.	ID4-	ID4-TDB0487
Ident No.	163 12 55 1 670
V max.	km/h	105 km/h
ID 2/ Basis Type (Brake)	ID2-	ID2-SNK300x200
AN (Order Number)
Tyre size	R single dual
Year of Construction (see vehicle papers)
Rigid axle
Self steering axle
Forced steering axle
Following information is necessary, only when axle type is unknown:
Axle cross
Camshaft diameter
Breake drum inner diameter
Brake pad width
Brake drum depth
Bearing marking (DIN-Norm)
Wheel bearing size or inner diameter:	Inner
Outer
Brake spider	Bolted	Forged part
Welded	Welded part
Adress / Contact Person
Please send the completed form per fax to:

+49 (0) 6095 301 - 260

Date:	Sign:

Type Plate up to mid-2004	Type Plate up from mid-2004

Type Plate up from 2007	Type Plate up from 2011

Identification where type plate is missing:

Serial no. of the axle on the right hand side to the direction of travel on the axle beam

Request for Replacement Type Plate

Process Instruction 111 33 0008 00 Type Plate / Document no. FoQM0073	03.2015

SAF‑HOLLAND GmbH • Hauptstr. 26 • D-63856 Bessenbach • Germany

Tel.: +49 (0) 6095 / 301 - 0 • Fax: +49 (0) 6095 / 301 - 260 • www.safholland.com

Anfrage zum Erstellen von Ersatztypenschildern

Zu Verfahrensanweisung Nummer 111 33 0008 00 Typschild / Formular-Nummer FoQM0071	03.2015

Service - Form

· Request for Replacement Type Plate

SAF-HOLLAND

2015-08-19

Polak, Adriane

SAF-HOLLAND